Cruise Control Components. Opel Sintra 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Cruise Control Module | Engine compartment, near the left strut tower | Antilock Brake System Component Views in ABS/Traction Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Release Switch | Mounted to the brake pedal support | Antilock Brake System Component Views in ABS/Traction Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Switch | Part of the turn signal switch, on the turn signal lever | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Stop Lamp Switch | Mounted to the brake pedal support | Antilock Brake System Component Views in ABS/Traction Control | Cruise Control Connector End Views in Cruise Control
Turn Signal Lever (Cruise Control Switch) | Left side of the steering column, part of the turn signal switch | -- | --
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G201 | Left side of the IP, secured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
S205 | IP harness, left side of the IP approximately 8 cm (3 in) from the hazard lamp/turn signal flasher breakout | -- | --
S266 | IP harness, left side of the IP approximately 24 cm (9 in) from the radio and the rear window wiper/washer multi-function switch breakout | -- | --