Parking Brake Cable Guide Replacement - Rear. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the park brake cable rear guide nut.
3. Remove the park brake cable rear guide.

### Installation Procedure

1. Install the park brake cable rear guide.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the park brake cable rear guide nut.

Tighten
Tighten the park brake cable rear guide nut to 14 N·m (124 lb in).

3. Lower the vehicle.