Instrument Panel Inflatable Restraint Module Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.
1. Disable the SIR system. Refer to Disabling the SIR System Disabling the SIR System .
2. Remove the RH insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges, and Console.
3. Remove the IP compartment and IP compartment lamp electrical connector. Refer to IP Compartment Replacement Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
4. Remove the inflatable restraint IP module pigtail harness clips from the IP carrier bracket.
5. Remove the inflatable restraint IP module mounting fasteners (4) that attach the inflatable restraint IP module to the cross-car beam.
6. Remove the inflatable restraint IP module fasteners (5) that attach the inflatable restraint IP module to the IP.
7. Remove the inflatable restraint IP module (1) from the vehicle.
8. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling, Shipping, and Scrapping .

### Installation Procedure

1. Install the inflatable restraint IP module (1) to the cross-car beam.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the inflatable restraint IP module fasteners (5) that attach the inflatable restraint IP module to the IP.

Tighten
Tighten fasteners to 10 N·m (89 lb in).

Use hand tools only to achieve fastener torque. This will prevent stripping of the replacement fastener.

3. Install the inflatable restraint IP module mounting fasteners (4) that attach the inflatable restraint IP module to the cross-car beam.

Tighten
Tighten fasteners to 10 N·m (89 lb in).

Use hand tools only to achieve fastener torque. This will prevent stripping of the replacement fastener.

4. Install the IP compartment lamp electrical connector and IP compartment. Refer to IP Compartment Replacement Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
5. Install the RH insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges, and Console.
6. Enable the SIR system. Refer to Enabling the SIR System Enabling the SIR System .