Electronic Brake and Traction Control Module Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the I/P sound insulator panel. Refer to Instrument Panel, Gages and Console in Body and Accessories.
2. Remove the EBCM/EBTCM electrical connectors (4).
3. Use pressure tabs in order to release the EBCM/EBTCM (1) from the EBCM/EBTCM bracket (2).

### Installation Procedure

1. Slide the EBCM/EBTCM (1) into the EBCM/EBTCM bracket (2) until pressure tabs secure the EBCM/EBTCM.
2. Install the EBCM/EBTCM electrical connectors (4).
3. Install the I/P sound insulator panel. Refer to Instrument Panel, Gages and Console in Body and Accessories.