Electronic Column Lock Module - Assemble - Off Vehicle. Opel Sintra 1999

For 1990-2009 cars

1. Install the electronic lock module assembly (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the three pan head tapping screws (2) into the electronic lock module assembly.

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

3. Install the park lock cable assembly (1) into the electronic lock module assembly.
4. Install the ignition and key alarm switch assembly (3) onto the electronic lock module assembly (2) and secure by using the 2 tapping screws.

Tighten
Tighten the screws to 4.7 N·m (42 lb in).

5. Slide the PASSKEY® III (2) onto the electronic lock module assembly (1).
6. Install the steering column tilt head assembly. Refer to Steering Column Tilt Head Housing - Assemble - Off Vehicle .