Ignition Coil. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the spark plug wires.
2. Remove the 2 screws securing coil to ignition control module.
3. Remove the coil assembly.

### Installation Procedure

1. Install the coil assembly.
2. Install the 2 screws.

Tighten
Tighten the screws to 4-5 N·m(40 lb. in.).

Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Install the spark plug wires.