Stabilizer Shaft Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front tire and wheel.

• | For vehicles with steel wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Chevrolet and Oldsmobile vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Pontiac vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

3. Remove the left and right stabilizer shaft insulators and brackets . Refer to Stabilizer Shaft Insulator Replacement .
4. Remove the left and right stabilizer shaft links. Refer to Stabilizer Shaft Link Replacement .
5. Remove the stabilizer shaft from the left side of the vehicle.

### Installation Procedure

1. Install the stabilizer shaft from the left side of the vehicle.
2. Install the left and right stabilizer shaft links. Refer to Stabilizer Shaft Link Replacement .
3. Install the left and right stabilizer shaft insulators and brackets. Refer to Stabilizer Shaft Insulator Replacement .
4. Install the left front tire and wheel.

• | For vehicles with steel wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Chevrolet and Oldsmobile vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

• | For Pontiac vehicles with aluminum wheels, refer to Tire and Wheel Removal and Installation in Tires and Wheels.

5. Lower the vehicle.