DTC B1025 Driver Deployment Loop Short to Voltage. Opel Sintra 1999

For 1990-2009 cars
SIR Components
SIR Schematics
Handling ESD Sensitive Parts Notice
SIR Caution

### Circuit Description

When you first turn the ignition switch to the RUN position, the inflatable restraint sensing and diagnostic module (SDM) performs tests to diagnose critical malfunctions within itself. Upon passing these tests, IGNITION, 23 VLR and the deployment loop voltages are measured to make sure they are within their respective normal voltage ranges. The SDM monitors the voltages at Driver Frontal Low terminal 2 and Passenger Frontal Low terminal 3 to detect shorts to B+ in the frontal air bag deployment loop circuits.

### Conditions for Setting the DTC

• | The voltage at Passenger Frontal Low terminal 3 is less than 3.5 volts.

• | The voltage at Driver Frontal Low terminal 2 is more than 4.5 volts for 500 milliseconds.

The CONTINUOUS MONITORING test checks for this DTC. This test occurs when IGNITION is within the normal operating voltage range.

• | POWER-ON When the malfunction is detected in this test, the RESISTANCE MEASUREMENT test will not be performed.

• | CONTINUOUS MONITORING

### Action Taken When the DTC Sets

• | The SDM sets a DTC B1025.

• | The SDM turns ON the AIR BAG warning lamp.

### Conditions for Clearing the DTC

• | Current DTC The voltage at Driver Frontal Low terminal 2 is less than 3.5 volts for 500 milliseconds.

• | History DTC

- | You issue a scan tool CLEAR CODES command.

- | Once 250 malfunction free ignition cycles have occurred.

### Diagnostic Aids

A short to B+ in the inflatable restraint steering wheel module circuit can cause an intermittent condition. Inspect CKT 347 and CKT 348 carefully for cutting or chafing. The diagnostic table directs the technician to note the entry value of DRIVER FRONTAL SENSELO. Comparing the value of DRIVER FRONTAL SENSELO can be helpful in determining if an intermittent condition exists.

When measurements are requested in this table, use J 39200 Digital Multimeter with the correct terminal adapter from J 35616 Connector Test Adapter Kit. When a check for proper connection is requested, refer to Intermittents and Poor Connections . When a wire, connector or terminal repair is requested, use J-38125 Terminal Repair Kit and refer to Wiring Repair .

### Test Description

The numbers below refer to the step numbers on the diagnostic table:

1. This step isolates the malfunction to one side of the inflatable restraint steering wheel module coil yellow 2-way connector.

2. This step determines if the inflatable restraint steering wheel module or the inflatable restraint steering wheel module coil is defective.

3. This step checks to see if there is a short to B+ in CKT 347.

4. This step determines if there is a short to B+ CKT 348 or if there is a malfunctioning SDM.

#### DTC B1025 Driver Frontal Air Bag Deployment Loop Short to Voltage

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the SIR Diagnostic System Check performed? | -- | Go to Step 2 | Go to SIR Diagnostic System Check

2

1. Turn the ignition switch to the OFF position.
2. Install the scan tool.
3. Turn the ignition switch to the RUN position.
4. Use the scan tool to request the SIR data list display.
5. Read and record on the repair order the driver frontal air bag low voltage DRIVER FRONTAL SENSELO.

Has the DRIVER FRONTAL SENSELO been read and recorded on the repair order?

--

Go to Step 3

--

3

1. Turn the ignition switch to the OFF position.
2. Disconnect the inflatable restraint steering wheel module coil and IP module yellow 2-way connectors.
3. Connect J 38715-A SIR Driver/Passenger Load Tool to the wiring harness connectors.
4. Turn the ignition switch to the RUN position.
5. Use the scan tool to request the SIR data list display.
6. Read the driver frontal air bag low voltage DRIVER FRONTAL SENSELO.

Is DRIVER FRONTAL SENSELO more than the specified value?

4.5 V

Go to Step 7

Go to Step 4

4

1. Turn the ignition switch to the OFF position.
2. Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .
3. Disconnect J 38715-A from the driver yellow 2-way wiring harness connector.
4. Connect the driver yellow 2-way connector.
5. Connect J 38715-A to the upper inflatable restraint steering wheel module coil connector on the steering column.
6. Turn the ignition switch to the RUN position.
7. Use the scan tool to request the SIR data list display.
8. Read the driver side low voltage DRIVER FRONTAL SENSELO.

Is DRIVER FRONTAL SENSELO more than the specified value?

4.5 V

Go to Step 6

Go to Step 5

5

1. Turn the ignition switch to the OFF position.
2. Replace the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .

Is the repair complete?

--

Go to Step 11

--

6

1. Turn the ignition switch to the OFF position.
2. Replace the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .

Is the repair complete?

--

Go to Step 11

--

7

1. Turn the ignition switch to the OFF position.
2. Disconnect the inflatable restraint sensing and diagnostic module (SDM). Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement .
3. Disconnect the J 38715-A .
4. Insert the J 42113 SIR Shorting Bar Tool into the SDM wiring harness connector above terminal 1 and terminal 2.
5. Turn the ignition switch to the RUN position.
6. Use the J 39200 Digital Multimeter (DMM) to measure the voltage between terminal A of the inflatable restraint steering wheel module coil yellow 2-way wiring harness connector and a known good ground.

Is the measured voltage less than the specified value?

1 V

Go to Step 9

Go to Step 8

8

1. Locate a short to B+ in CKT 347.
2. Replace the short to B+ in CKT 347.

Is the repair complete?

--

Go to Step 11

--

9 | Use the J 39200 Digital Multimeter (DMM) to measure the voltage between terminal B of the inflatable restraint steering wheel module coil yellow 2-way wiring harness connector and a known good ground. Is the resistance reading less than the specified value? | 1 V | Go to Sensing and Diagnostic Module Integrity Check | Go to Step 10

10

1. Locate a short to B+ in CKT 348.
2. Replace the short to B+ in CKT 348.

Is the repair complete?

--

Go to Step 11

--

11 | Reconnect all the SIR system components, make sure all the components are properly mounted. Have all the SIR components been reconnected and properly mounted? | -- | Go to Step 12 | --
12 | Use the scan tool to clear all current and history SIR DTCs. Have all current and history SIR DTCs been cleared? | -- | Go to SIR Diagnostic System Check | --