Engine Controls Components. Opel Sintra 1997

For 1990-2009 cars

#### ENGINE COMPONENT LOCATION TABLE

Name | Location | Locator View (8A Cell 201 Figure #) | Connector End View (8A) | Group No.
--- | --- | --- | --- | ---
A/C Compressor Clutch Coil | Part of A/C compressor | 7 | -- | --
A/C Refrigerant Pressure Sensor | LH side of engine compartment, below accummlator, below air cleaner assembly | 65 | -- | --
Automatic Transaxle | Lower LH side of engine compartment | 7 | -- | --
Body Control Module (BCM) | Below RH side of I/P, right of I/P compartment | 17 | 51-2 | --
Camshaft Position (CMP) Sensor | Engine compartment, RH side of engine, above A/C compressor clutch | 3 | -- | --
Crankshaft Position (CKP) Sensor (7X) | Lower rear of engine | -- | -- | --
Crankshaft Position (CKP) Sensor (24X | RH side of engine, at end of crankshaft, behind harmonic balancer | 7 | -- | --
Cruise Control Module | Engine compartment, near LH strut tower | 11 | 34-1 | --
Data Link Connector (DLC) | Below steering column, bottom of knee bolster | 14 | 50-1 | --
Driver Information Display | In roof console | -- | 86-1 | --
Electronic Brake Traction Control Module (EBTCM) | LH side of I/P, above park brake cable bracket | 13 | 5E2 | --
Engine Coolant Fan Motor #1 (RH) | Mounted to rear RH side of radiator | 1 | -- | --
Engine Coolant Fan Motor #2 (LH) | Mounted to rear LH side of radiator | 1 | -- | --
Engine Coolant Temperature (ECT) Sensor | LH side top of engine | -- | -- | --
Engine Oil Level Indicator Switch | Center of engine oil pan | 62 |  |
Evaporative Emmissions (EVAP) Canister Purge Solenoid valve | Top rear of engine, below ignition control module | 4 | -- | --
Evaporative Emissions (EVAP) Cannister Purge Vacuum Switch | Top rear of engine, below ignition control module | 4 | -- | --
Exhaust Gas Recirculation (EGR) Valve | Upper LH side of engine | 6 | 202-35 | --
Fuel Injectors | Top of engine at each cylinder intake port | -- | -- | --
Fuel Pump Motor | Mounted inside fuel tank | -- | -- | --
Fuel Pump Prime Connector | One cavity connector, branching out of engine wiring harness, near battery | -- | -- | --
Fuel Tank | Below LH side, middle of vehicle | 55 | -- | --
Fuse Block | RH side of I/P, in RF door opening | -- | -- | --
Generator (K68) | Top rear RH side of engine | 5 | 202-36 | --
Generator (KG9) | Top rear RH side of engine | 5 | 202-36 | --
Heated Oxygen Sensor (HO2S) #1 | Rear of engine, in exhaust manifold | 4 | 202-37 | --
Heated Oxygen Sensor (HO2S ) #2 | In exhaust system, behind catalytic converter | 54 | 202-37 | --
Heater-A/C Control | Center of I/P, below radio | 24 | 202-38 | --
Idle Air Control (IAC) Valve | Top of engine, front of throttle assembly | 6 | 202-38 | --
Ignition Control Module (ICM) | Top center rear of engine | 4, 5 | 202-38 | --
Instrument Cluster | LH side of I/P | 16 | 81-6 | --
Intake Air Temperature (IAT) Sensor | LF of engine compartment, on air intake duct, near throttle body | 6 | -- | --
Knock Sensor (KS) | Front of engine, above starter | 7 | -- | --
Manifold Absolute Pressure (MAP) Sensor | RH top of engine | -- | -- | --
Mass Air Flow (MAF) Sensor | LH front of engine compartment, in air cleaner duct | 6 | -- | --
Powertrain Control Module (PCM) | Engine compartment, secured in air cleaner assembly | 12 | Refer to Engine Controls Connector End Views | --
Radio | Center of I/P console | 27 | 105-5 |
Rear Side Door Actuator Motor | RH quarter panel, above wheelhouse | 34 | 137-2 | --
Stop Lamp Switch | Mounted to brake pedal support | 19 | 202-53 | --
Throttle Position (TP) Sensor | Top of engine, on throttle assembly | 6 | -- | --
Transaxle Range Switch | Rear LH side of engine compartment, mounted to top of transaxle | 7 | 202-54 | --
Underhood (UH) Electrical Center | Engine compartment, front of RH wheelhouse, above battery | 1,8 | 202-55 | --
Vehicle Speed Sensor (VSS) | Lower RR of engine compartment, mounted to RH side of transaxle | 62 | -- | --
C101 (10 cavities) | I/P wiring harness to engine wiring harness, in lower LH side of engine compartment, next to C103 | 11 | 202-0 | --
C102 (10 cavities) | Engine wiring harness to fuel injector wiring harness, top of engine, near generator next to C108 | 5 | 202-1 | --
C105 (2 cavities) | Engine wiring harness to engine coolant fan wiring harness, behind engine coolant fan #2 (LH) | 1 | 202-2 | --
C108 (3 cavities) | Engine wiring harness to fuel injector wiring harness, top of engine, near generator, next to C102 | 5 | 202-3 | --
C200 (56 cavities) | I/P wiring harness to RH side of body wiring harness, behind RH side of I/P compartment, below P100 | 33 | 202-6 | --
C305 (12 cavities) | Body wiring harness to electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath vehicle behind driver seat | 55 | 202-19 | --
C308 (23 cavities) | Body wiring harness to dome lamp wiring harness, inside RH B-pillar, behind lower trim | 32 | 202-20 |
G111 | Engine compartment, left of starter, along with battery ground | 7 | -- | --
G113 | Engine compartment, left of starter, along with battery ground | 7 | -- | --
G117 | Engine compartment, left and above starter, near connector C111 to automatic transaxle | 7 | -- | --
G200 | RH side of I/P, secured on underside of cross car beam, left of heater-A/C vent | 28 | -- | --
G301 | Secured to inside of lower LH B pillar | 36 | -- | --
P100 | On RH side of bulkhead, left of RH strut tower | 2 | -- | --
P101 | On LH side of bulkhead, right of LH strut tower | 11 | -- | --
S105 | Engine harness, top RH side radiator approximately 20 cm (8 in) from engine coolant fan #1 (RH) motor breakout | -- | -- | --
S106 | Engine harness, front LH side of engine compartment approximately 10 cm (4 in) from powertrain control module (PCM) | -- | -- | --
S107 | Engine harness, center of engine approximately 4 cm (1 in) from camshaft position sensor breakout | -- | -- | --
S109 | Fuel injector harness, center of engine approximately 12 cm (5 in) from fuel injector #1 | -- | -- | --
S115 | Automatic transaxle harness, inside automatic transaxle housing approximately 42 cm (17 in) from automatic transaxle fluid temperature sensor | -- | -- | --
S122 | Engine harness, top LH side of radiator approximately 25 cm (10 in) from engine coolant fan #1 (RH) motor breakout | -- | -- | --
S146 | Engine harness, center of engine approximately 10 cm (4 in) from engine coolant fan #1 (RH) motor breakout | -- | -- | --
S155 | Engine harness, front of engine approximately 14 cm (6 in) from knock sensor (KS) breakout | -- | -- | --
S209 | I/P harness, center of I/P approximately 8 cm (3 in) from security indicator lamp | -- | -- | --
S211 | I/P harness, LH side of I/P approximately 37 cm (15 in) from hazard lamp/turn signal flasher breakout | -- | -- | --
S237 | I/P harness, RH side of I/P approximately 4 cm (2 in) from C201 breakout | -- | -- | --
S238 | I/P harness, center of I/P approximately 80 cm (31 in) from the cigar lighter connector | -- | -- | --
S264 | I/P harness, RH side of I/P approximately 16 cm (6 in) from relay center breakout | -- | -- | --
S328 | Body harness, RH B pillar approximately 14 cm (6 in) from G302 breakout | -- | -- | --