Rear Side Door Window Bumper Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Use a heat gun in order to heat the sliding window bumpers.

Hold the heat gun 152 mm (6 in) from the surface.

2. Use a circular motion in order to apply heat for approximate 30 seconds.
3. Use a flat-bladded tool in order to peel the window bumpers from the panel surface.

Do not damage the paint.

4. Clean the body panel.

Use oil-free naphtha or alcohol.

### Installation Procedure

1. Warm the body panel with a heat lamp or a heat gun to a minimum of 21°C (70°F).
2. Peel the backing from the front end of the window bumpers.

Do not touch the adhesive backing.

3. Press the window bumpers to the body.
4. Hand roll the window bumpers to the body in order to ensure proper adhesion.