Transmission Fluid Filler Tube Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the indicator.
2. Remove the nut from the upper fluid filler tube bracket.
3. Raise and suitably support the vehicle. Refer to

   Caution: To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle at the opposite end from which components are being removed. This will reduce the possibility of the vehicle falling off the hoist.

   in General Information.
4. Remove the three-way catalytic converter pipe. Refer to Engine Exhaust.
5. Remove the power steering gear heat shield. Refer to Power Steering Gear and Pump.
6. Remove the bolt from the lower fluid filler tube bracket.
7. Remove the fluid filler tube.

### Installation Procedure

Important: Do NOT place the seal on the tube when installing the tube or damage to the seal will result.

1. Install the seal into the transaxle.
2. Position the fluid filler tube.
3. Install the bolt through the lower fluid filler tube bracket.

Tighten
Tighten the lower fluid filler tube bracket bolt to 13 N·m (115 lb in). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
4. Install the power steering gear heat shield. Refer to Power Steering Gear and Pump.
5. Install the three-way catalytic converter pipe. Refer to Engine Exhaust.
6. Lower the vehicle.
7. Install the nut to the upper fluid filler tube bracket.

Tighten
Tighten the upper fluid filler tube bracket nut to 13 N·m (115 lb in).

8. Install the indicator.
9. Adjust the fluid level.
10. Inspect for proper completion of the repairs.
11. Inspect for proper fluid level.
12. Inspect for fluid leaks.