Accessory Port Replacement - Rear. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the rear accessory panel access door from the left rear quarter trim panel.
2. Use a flat-bladed tool to pry out retaining tab on accessory panel.
3. Pull accessory panel from the quarter trim panel.
4. Disconnect the electrical connector from the accessory port.
5. Unscrew retaining sleeve from accessory port.
6. Remove the accessory port from the panel.

### Installation Procedure

1. Install the accessory port to the panel.
2. Install the retaining sleeve to the accessory port and tighten sleeve.
3. Connect the electrical connector to the accessory port.
4. Align retaining tabs on the accessory panel with the holes in the rear quarter trim panel.
5. Align the retaining tab of the accessory panel with the slot in the rear quarter trim panel and push access panel into quarter trim panel.
6. Install access panel door.