DOOR AJAR Message Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---

1

1. Disconnect connector C203.
2. Connect a fused (3 amp) jumper between the connector C203 terminal C6 (leading towards the instrument cluster) and ground.
3. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 2

Go to Step 30

2

1. Reconnect connector C203.
2. Disconnect connector C303.
3. Connect the fused (3 amp) jumper between the connector C303 terminal H (leading towards the instrument cluster) and ground.
4. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 3

Go to Step 31

3

1. Reconnect connector C303.
2. Disconnect the LF door lock connector C1.
3. Connect the fused (3 amp) jumper between the LF door lock connector terminal B (leading towards the instrument cluster) and ground.
4. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 4

Go to Step 32

4 | Connect the fused (3 amp) jumper between the LF door lock connector C1 terminal B and terminal D. Is the DOOR AJAR indicator on? | -- | Go to Step 5 | Go to Step 6

5

1. Reconnect the LF door lock connector.
2. Turn the ignition switch to the RUN position.

With the LF door open, is the DOOR AJAR indicator on?

--

Go to Step 8

Go to Step 7

6 | Repair poor connection or open in circuit 750 between the LF door lock connector C1 terminal D and G302. Has the repair been made and the system rechecked? | -- | System OK | --
7 | Replace the LF door lock. Refer to Front Side Door Lock Replacement in Doors. Has the repair been made and the system rechecked? | -- | System OK | --

8

1. Disconnect connector C302.
2. Connect a fused (3 amp) jumper between connector C302 terminal H and ground.
3. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 9

Go to Step 33

9

1. Reconnect connector C302.
2. Disconnect the RH door lock connector C1.
3. Connect the fused (3 amp) jumper between the RF door lock connector C1 terminal C and ground.
4. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 10

Go to Step 34

10

1. Connect the fused (3 amp) jumper between the RF door lock connector C1 terminal C and terminal A.
2. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 11

Go to Step 12

11

1. Reconnect the RF door lock connector C1.
2. Turn the ignition switch to the RUN position.

With the RF door open, is the DOOR AJAR indicator on?

--

Go to Step 14

Go to Step 13

12 | Repair poor connection or open in circuit 750 between the RF door lock connector C1 terminal A and G302. Has the repair been made and the system rechecked? | -- | System OK | --
13 | Replace the RF door lock. Refer to Front Side Door Lock Replacement in Doors. Has the repair been made and the system rechecked? | -- | System OK | --

14

1. Disconnect connector C402.
2. Connect a fused (3 amp) jumper between connector C402 terminal E and ground.
3. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 15

Go to Step 35

15

1. Reconnect connector C402.
2. Disconnect the liftgate lock connector C1.
3. Connect the fused (3 amp) jumper between the liftgate door lock connector C1 terminal B and ground.
4. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on

--

Go to Step 16

Go to Step 36

16

1. Connect the fused (3 amp) jumper between the liftgate lock connector C1 terminal B and terminal D.
2. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 17

Go to Step 18

17

1. Reconnect the liftgate lock connector C1.
2. Turn the ignition switch to the RUN position.

With the liftgate open, is the DOOR AJAR indicator on?

--

Go to Step 20

Go to Step 19

18 | Repair poor connection or open in circuit 450 between the liftgate lock connector C1 terminal D and G401. Has the repair been made and the system rechecked? | -- | System OK | --
19 | Replace the liftgate lock. Refer to Liftgate Lock Cylinder Replacement in Body Rear End. Has the repair been made and the system rechecked? | -- | System OK | --

20

1. Disconnect the RH sliding door jamb switch connector.
2. Connect a fused (3 amp) jumper between the RH sliding door jamb switch connector terminal A and ground.
3. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 21

Go to Step 37

21

1. Connect the fused (3 amp) jumper between the RH sliding door jamb switch connector terminal A and terminal C.
2. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 22

Go to Step 23

22

1. Reconnect the RH sliding door jamb switch connector.
2. Turn the ignition switch to the RUN position.

With the RH sliding door open, is the DOOR AJAR indicator on?

--

System OK (if equipped with LH sliding door Go to Step 25 )

Go to Step 24

23 | Repair poor connection or open in circuit 750 between the RH sliding door jamb switch connector terminal C and G302. Has the repair been made and the system rechecked? | -- | System OK | --
24 | Replace the RH sliding door jamb switch. Refer to Door Jamb Switch Replacement - Sliding Door in Doors. Has the repair been made and the system rechecked? | -- | System OK | --

25

1. Disconnect the LH sliding door jamb switch connector.
2. Connect a fused (3 amp) jumper between the LH sliding door jamb switch connector terminal A and ground.
3. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 26

Go to Step 38

26

1. Connect the fused (3 amp) jumper between the LH sliding door jamb switch connector terminal A and terminal C.
2. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 27

Go to Step 28

27

1. Reconnect the LH sliding door jamb switch connector.
2. Turn the ignition switch to the RUN position.

With the LH sliding door open, is the DOOR AJAR indicator on?

--

System OK

Go to Step 29

28 | Repair poor connection or open in circuit 750 between the LH sliding door jamb switch connector terminal C and G302. Has the repair been made and the system rechecked? | -- | System OK | --
29 | Replace the LH sliding door jamb switch. Refer to Door Jamb Switch Replacement - Sliding Door in Doors. Has the repair been made and the system rechecked? | -- | System OK | --

30

1. Using a fused (3 amp) jumper, backprobe between the instrument cluster connector C1 terminal G and ground.
2. Turn the ignition switch to the RUN position.

Is the DOOR AJAR indicator on?

--

Go to Step 39

Go to Step 40

31 | Repair poor connection or open in circuit 804 between the connector C203 terminal C6 and connector C303 terminal H. Has the repair been made and the system rechecked? | -- | System OK | --
32 | Repair poor connection or open in circuit 804 between the LF door lock connector C1 terminal B and connector C303 terminal H. Has the repair been made and the system rechecked? | -- | System OK | --
33 | Repair poor connection or open in circuit 804 between S308 and connector C302 terminal H. Has the repair been made and the system rechecked? | -- | System OK | --
34 | Repair poor connection or open in circuit 804 between the RF door lock connector C1 terminal C and C302 terminal H. Has the repair been made and the system rechecked? | -- | System OK | --
35 | Repair poor connection or open in circuit 804 between S308 and connector C402 terminal E. Has the repair been made and the system rechecked? | -- | System OK | --
36 | Repair poor connection or open in circuit 804 between the liftgate lock connector C1 terminal B and C402 terminal E. Has the repair been made and the system rechecked? | -- | System OK | --
37 | Repair poor connection or open in circuit 804 between the RH sliding door jamb switch connector terminal A and S308. Has the repair been made and the system rechecked? | -- | System OK | --
38 | Repair poor connection or open in circuit 804 between the LH sliding door jamb switch connector terminal A and S308. Has the repair been made and the system rechecked? | -- | System OK | --
39 | Repair poor connection or open in circuit 804 between the instrument cluster connector C1 terminal G and C203 terminal C6. Has the repair been made and the system rechecked? | -- | System OK | --

40

1. Check the DOOR AJAR indicator bulb and bulb connection.
2. If OK, replace the instrument cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console.

Has the repair been made and the system rechecked?

--

System OK

--