Driver Information Center (DIC) Display Does Not Retain Last Request Mode. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for a poor connection or open in circuit 640 between the driver information display harness connector terminal 14 and the underhood accessory wiring junction block harness connector C2 terminal F7. Is there a poor connection or open in circuit 640? | -- | Go to Step 2 | Go to Step 3
2 | Repair the poor connection or open in circuit 640 between the driver information display harness connector terminal 14 and the underhood wiring junction block harness connector C2 terminal F7. Has the repair been made and the system rechecked? | -- | System OK | --
3 | Replace the driver information display. Refer to Driver Information Center Replacement in Instrument Panel, Gauges and Console. Has the repair been made and the system rechecked? | -- | System OK | --