Front Side Door Roof Drip Weatherstrip Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Pull the front door roof drip weather-strip from the pinch-weld flange.
2. Clean all of the adhesive from the pinch-weld flange.

### Installation Procedure

Important: A mastic/sealer/glue is inside the new front door opening weather-strip. If you are using a new front door opening weather-strip, do not use any weather-strip adhesive.

If the old front door roof drip weather-strip is reused, apply weather-strip adhesive.
1. Align the front door roof drip weather-strip to the pinch-weld flange at the upper C-pillar.
2. Work the weather-strip forward and down the A-pillar.
3. Tuck the forward end of the front roof drip weather-strip under the fender.