Outside Mirrors System Check. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Move the mirror select switch to the LEFT position.
2. Operate the mirror position switch in the UP and DOWN positions.
3. Operate the mirror position switch in the LEFT and RIGHT positions.

1. The LH outside rearview mirror moves smoothly upward and downward.
2. The LH outside rearview mirror moves smoothly to the left and the right.

• | Power mirrors inop in up/down direction-one. Go to Power Mirrors Inoperative in Up/Down Direction - One .

• | One mirror inop in left/right direction-one. Go to Power Mirrors Inoperative in Left/Right Direction - One .

2

1. Move the mirror select position to the RIGHT position.
2. Operate the mirror position switch in the UP and DOWN positions.
3. Operate the mirror position switch in the LEFT and RIGHT positions.

1. The RH outside rearview mirror moves smoothly upward and downward.
2. The RH outside rearview mirror moves smoothly to the left and the right.

• | Power mirrors inop. Go to Power Mirrors Inoperative .

• | Power mirrors inop-one. Go to Power Mirrors Inoperative - One .

• | Power mirrors inop in up/down direction-one. Go to Power Mirrors Inoperative in Up/Down Direction - One .

• | Power mirrors inop in left/right direction-one. Go to Power Mirrors Inoperative in Left/Right Direction - One .