Evaporative Emission Vacuum Switch. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector and vacuum hoses from the EVAP vacuum switch.
2. Bend the tab on the switch mounting bracket in order to remove the switch.

### Installation Procedure

1. Bend tab on mounting bracket to retain the EVAP Vacuum switch.
2. Install the EVAP vacuum switch to bracket.

- | Once installed pull on the vacuum switch to ensure that the part will be held in place.

3. Connect the electrical connector and hoses to the EVAP vacuum switch.