Hazard Lamps Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the HAZARD fuse. Is the fuse open? | -- | Go to Step 2 | Go to Step 3
2 | Repair a short to ground in CKT 1840. Is the repair complete? | -- | Go to Exterior Lights System Check | --

3

1. Turn the ignition to the RUN position.
2. Use a test lamp in order to backprobe between C201 terminal E8 and ground.

Did the test lamp light?

--

Go to Step 5

Go to Step 4

4

Repair the following conditions in CKT 1840:

• | A faulty connection

• | An open circuit

Is the repair complete?

--

Go to Exterior Lights System Check

--

5 | Replace the turn signal switch. Is the repair complete? | -- | Go to Exterior Lights System Check | --