PAINT CODES AND REFINISH INFORMATION. Pontiac LeMans 1988

For 1990-2009 cars

# PAINT CODES AND REFINISH INFORMATION

#### Models Affected: 1988 LeMANS

The LeMans assembly plant uses PPG (Ditzler) Paint Systems, and will be painting vehicles with basecoat/clearcoat and conventional enamels. Metalic colors employ a basecoat/clearcoat system and are designated "Metalic C/C" on the chart. All other colors are enamel and do not have a clearcoat applied.

The WA codes listed on the S.P.I.D. Label located on the inside of the deck lid are correct and should be used to properly identify the paint on the vehicle.

#### PONTIAC LeMANS REFINISH PAINT

Pontiac Sales Daewoo # Sherwin- (BASF) Sales WA Color on Header Williams (PPG) RM Martin Code No. No. Name Panel Acme/Rogers Ditzler DuPont Inmont Senour ------- --- ---- --------- ----------- ------- ------ ------ ------ 11U 9507 White 11L 38137 90452 K8878 18385 38137

13U 9511 Silver 86L 38118 34312 K8812 18386 38118 Metallic C/C

19U 9509 Black 80L F10B-1738 9667 99 18387 8800 80/4080 22U 9512 Lt. Blue 28L 38119 16375 K8813 18388 38119 Metallic C/C

72U 9510 Medium 71L 38134 72991 K8880 18390 38134 Maroon

81U 9508 Bright 76L 38135 72990 K8881 18391 38135 Red

95U 9513 Light 50L 38136 34313 K8882 18392 38136 Champagne Metallic C/C

(15) 8573 Medium --- 38138 34362 K8883 18393 38138 Gray Metallic

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.