PAINT CODES REFINISH INFORMATION. Pontiac LeMans 1989

For 1990-2009 cars

# PAINT CODES REFINISH INFORMATION

#### ModelsAffected: 1989 LEMANS

The LeMans assembly plant uses PPG (Ditzler) Paint Systems, and will be painting vehicles with basecoat/clearcoat and conventional enamels. Metalic colors employ a basecoat/clearcoat system and are designated "Metalic C/C" on the chart. All other colors are enamel and do not have a clearcoat applied.

The WA codes listed on the S.P.I.D. Label, located in the trunk under the carpet at the left rear, should be used to properly identify the paint on the vehicle.

DAEWOO PONTIAC NUMBER SHERWIN- SALES SALES ON WILLIAMS (BASF) CODE WA COLOR HEADER ACME/ (PPG) RM MARTIN NUMBER NO. NAME PANEL ROGERS DITZLER DUPONT INMONT SENOUR ------ --- ----- ------ --------- ------- ------ ------ ------ 10U 9573 Bright 10L 40412 90656 H9014 19156 40412 White

13U 9511 Silver 86L 38118 34312 K8812 18386 38118 Metallic C/C

19U 9509 Black 8OL FlOB-1738 9667 99 18387 8800

24U 9574 Bright 12L 40413 16820 H9015 19157 40413 Blue Metallic C/C

72U 9510 Medium 71L 38134 72991 K8880 18390 38134 Maroon

74U 9575 Flame 75L 40414 73963 H9016 19158 40414 Red Metallic C/C

95U 9513 Light 5OL 38136 34313 K8882 18392 38136 Champagne Metallic C/C

(15) 8573 Meduim -- 38138 34362 K8883 18393 38138 Gray Metallic

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.