CHASSIS SPRING SHIMS UPPER/LOWER P/N'S. Pontiac LeMans 1981

For 1990-2009 cars

# CHASSIS SPRING SHIMS UPPER/LOWER P/N'S

1977 THROUGH 1985 REAR WHEEL DRIVE VEHICLES

Spring shims for minor correction of low trim height are available from GMWDD. The shims can be used on 1977 through 1985 rear wheel drive vehicles.

These shims are 1/8" thick, and no more than two (2) are to be used at each spring location. When used on a front spring, the vehicle's trim height at the wheel opening will be increased approximately two (2) times the thickness of the shim. When used on a rear spring, the trim height will be increased approximately the same amount as the thickness of the shims.

Part Description Part Number ---------------- ----------- Shim, *Front Spring Upper 25524879

Shim, *Rear Spring Lower 25524880

*USE SHIMS ONLY AT LOCATION ON SPRING, AS SPECIFIED ABOVE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.