TRANS. UNIT REPAIR REVISION INTERMEDIATE BAND ADJUSTMENT. Pontiac LeMans 1983

For 1990-2009 cars

# TRANS. UNIT REPAIR REVISION INTERMEDIATE BAND ADJUSTMENT

THE FOLLOWING IS A REVISION TO THE AUTOMATIC TRANSMISSION 250C UNIT REPAIR SECTION, PAGE 250C-25, STEP NO. 28 SHOULD BE REVISED TO READ: AFTER PUMP ASSEMBLY IS COMPLETELY INSTALLED, ADJUST INTERMEDIATE BAND. TIGHTEN ADJUSTING SCREW TO 3.7 N.M (30 IN. LBS.) AND THEN BACKOFF 3 COMPLETE TURNS. WHILE HOLDING SCREW IN POSITION, TIGHTEN LOCK NUT TO 20.3 N.M (15 FT. LBS.) (FIGURE 250C-90)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.