HARSH 1-2 AND/0R 3-4 SHIFTS ALL MODEL THM 200-4R TRANS. Pontiac LeMans 1983

For 1990-2009 cars

# HARSH 1-2 AND/0R 3-4 SHIFTS ALL MODEL THM 200-4R TRANS

#### MODELS AFFECTED: Grand Prix, Bonneville, Parisienne,Parisienne Wagon

SERVICE PROCEDURE -

1. On the BQ and OM model transmissions remove the control valve body assembly and the 3-4 accumulator spring from the transmission and replace with the control valve body assembly and the 3-4 accumulator spring provided in the service package.

2. On the BT, and BY model transmissions remove the following parts and replace them with the parts which are contained in the service package.

A. Control Valve Body Assembly B. * 3-4 Accumulator Spring C. 1-2 Accumulator Spring D. Control Valve Body Spacer Plate E. Pressure Regulator Valve Spring F. Intermediate Servo Cushion Spring

#### NOTE: THE 3-4 ACCUMULATOR SPRING ON THE BT AND BY MODEL TRANSMISSIONS IS TO BE REMOVED AND DISCARDED. THE 3-4 ACCUMULATOR PISTON IS TO BE ASSEMBLED AS SHOWN IN FIGURES 1 AND 2.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.