WAGON TAILGATE GLASS BALL STUD REPAIR INFORMATION. Pontiac LeMans 1980

For 1990-2009 cars

# WAGON TAILGATE GLASS BALL STUD REPAIR INFORMATION

IN THE EVENT THAT THE TAILGATE GLASS BALL STUD BECOMES LOOSE, IT IS NOT NECESSARY TO REPLACE THE COMPLETE REAR WINDOW ASSEMBLY.

THE FOUR TAILGATE WINDOW MOULDING PIECES ARE SERVICED SEPARATELY (GROUP 12. 180 MOULDING, TAILGATE WINDOW GLASS). INSTRUCTIONS FOR PERFORMING THIS REPAIR CAN BE FOUND IN THE 1981 FISHER BODY MANUAL ON PAGE 7-36.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.