ENGINE OIL PAN GASKET 4.3L V-6 AND 5.7L V-8. Pontiac LeMans 1983

For 1990-2009 cars

# ENGINE OIL PAN GASKET 4.3L V-6 AND 5.7L V-8

THE OIL PAN GASKET ON THE ENGINES LISTED ABOVE CONTAIN A STAMPED STEEL CORE WITH CORK BONDED TO EACH SIDE. IF THE CORK COMES OFF, THE SHARP STEEL EDGE WILL BE EXPOSED.CAUTION: CARE SHOULD BE TAKEN WHEN HANDLING THIS GASKET TO AVOID THE POSSIBILITY OF PERSONAL INJURY.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.