BARO SENSOR RELOCATION INFORMATION. Pontiac LeMans 1982

For 1990-2009 cars

# BARO SENSOR RELOCATION INFORMATION

THE BARO SENSOR ON THE 1982 CUTLASS SUPREME HAS BEEN RELOCATED INSIDE THE VEHICLE UNDER THE INSTRUMENT PANEL NEAR THE ECM. IT IS THE SAME SENSOR AS 1981 AND CONNECTS TO THE HARNESS WITH A SHORT JUMPER HARNESS. THE EGR CUTOUT RELAY IS MOUNTED WHERE THE BARO SENSOR MOUNTED IN 1981, ON THE RIGHT INNER FENDER UNDER THE HOOD.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.