SERVICE MANUAL UPDATE MAGNETIC TIMING ADJUSTMENT. Pontiac LeMans 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE MAGNETIC TIMING ADJUSTMENT

#### Models Affected: 1988-90 LEMANS WITH 1.6L (VIN 6)

When utilizing magnetic probe timing equipment to check or adjust ignition timing on Lemans equipped with 1.6L (VIN 6) engines (as mentioned in Sections 6E2 and 6D4 of the 1988-90 Service manuals), consult the timing equipment manufacturers instructions for the correct offset adjustment for this engine. If the standard General Motors offset adjustment is used, ignition timing could be set incorrectly, resulting in poor performance and reduced fuel economy.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.