WINDSHIELD & BACK WINDOW PROPER GLASS INSTALLATION. Pontiac Sunbird 1984

For 1990-2009 cars

# WINDSHIELD & BACK WINDOW PROPER GLASS INSTALLATION

"Please discard previous bulletin 84-10-2 - additional information added to title "

Windshields on all 2000 style vehicles and back windows on "J-27-69" styles will use spacers to maintain proper dimensions of the glass in its respective opening.

The spacer (part number 20481008) is mounted on the pinch weld flange in five (5) locations for windshields and five (5) locations on back windows (see illustration).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.