SMU-SEC. 10-5 REVISED WASHER NOZZLE & TOP VENT SCREEN REM.. Pontiac Sunbird 1991

For 1990-2009 cars

# SMU-SEC. 10-5 REVISED WASHER NOZZLE & TOP VENT SCREEN REM.

#### APPLICATION:

1990-94 CHEVROLET CAVALIER 1990-94 PONTIAC SUNBIRD

THIS BULLETIN REVISES THE SHROUD TOP VENT GRILL PANEL REMOVAL PROCEDURE FOUND IN THE APPLICABLE SERVICE MANUAL, SECTION 10-5.

WHENEVER THE SHROUD TOP VENT GRILL PANEL IS REMOVED OR THE WINDSHIELD WASHER NOZZLE IS TO BE REMOVED, THE FOLLOWING REVISED PROCEDURE SHOULD BE USED TO PREVENT NOZZLE DAMAGE.

REMOVE OR DISCONNECT ====================

1. USING A 7MM DEEP SOCKET, REMOVE NOZZLE SCREW TO TOP VENT GRILL PANEL. (REFER TO ILLUSTRATION). 2. CAREFULLY REMOVE WASHER HOSE FROM NOZZLE USING A GENTLE TWISTING MOTION. 3. REMOVE NOZZLE FROM VEHICLE. 4. WIPER ARM ASSEMBLIES. 5. OPEN HOOD TO FULL OPEN POSITION, THEN REMOVE AIR INLET GRILL PANEL SCREWS. 6. SHROUD TOP VENT GRILL PANEL. 7. SHROUD SCREEN FROM PANEL. 8. HOOD SEAL LACE FROM PANEL.

INSTALL OR CONNECT ==================

1. HOOD SEAL LACE FROM PANEL. 2. SHROUD SCREEN FROM PANEL. 3. SHROUD TOP VENT GRILL PANEL. 4. AIR INLET GRILL PANEL SCREWS. 5. WIPER ARM ASSEMBLIES. 6. WASHER NOZZLE TO PANEL. 7. WASHER HOSE. 8. SCREW TO NOZZLE.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.