REVISED TORQUE SPEC. FOR FRONT HUB/BEARING ASSEMBLY. Pontiac Sunbird 1984

For 1990-2009 cars

# REVISED TORQUE SPEC. FOR FRONT HUB/BEARING ASSEMBLY

#### VEHICLES AFFECTED: 1983-84 'J' Series Vehicles

The torque value shown in the 1983-84 'J' Series Service Manual 85 N.m (63 ft. lbs.), for subject component should read 55 N.m (40 ft. lbs.). (Refer to Section 3C.)

Please make note of the change in your copy of the Service Manual.

The above information will be included in the bound 1984 Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.