SERVICE MANUAL UPDATE SEC. 6A1 CRANKSHAFT POSITION SENSOR. Pontiac Sunbird 1993

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6A1 CRANKSHAFT POSITION SENSOR

#### Subject: SERVICE MANUAL UPDATE - SECTION 6A1 CRANKSHAFT POSITION SENSOR RELUCTOR RING SERVICE PROCEDURE

#### Models Affected: 1992 SUNBIRD MODELS (RPO LE4)

The following procedure should be used for servicing the Crankshaft Position Sensor Reluctor Ring. This procedure should be added to the 1992 Sunbird Service Manual - Section 6A1.

The following procedure should be used for servicing the Crankshaft Position Sensor Reluctor Ring. This procedure should be added to the 1992 and 1993 Pontiac Sunbird Service Manual - Section 6A1.

CRANKSHAFT POSITION SENSOR RELUCTOR RING

Remove or Disconnect

1. Crankshaft, refer to "Crankshaft" in this section.

2. Reluctor ring Torx screws.

3. Reluctor ring.

Install or Connect

1. Reluctor ring.

2. Torx screws.

Tighten

o Screws to 14 N-m (124 lb. in.).

3. Crankshaft, refer to "Crankshaft" in this section.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.