SQUEAK BETWEEN DOOR HEADER AND AUXILIARY WEATHERSTRIP. Pontiac Sunbird 1994

For 1990-2009 cars

# SQUEAK BETWEEN DOOR HEADER AND AUXILIARY WEATHERSTRIP

#### SUBJECT: SQUEAK BETWEEN DOOR HEADER AND AUXILIARY WEATHERSTRIP (APPLY SQUEAK REDUCTION TAPE)

#### MODELS: 1993-94 CHEVROLET CAVALIER 1993-94 PONTIAC SUNBIRD

#### CONDITION:

SOME OWNERS MAY COMMENT ON A SQUEAK BETWEEN THE DOOR HEADER AND AUXILIARY WEATHERSTRIP.

#### CAUSE:

SQUEAK IS CAUSED BY CONTACT BETWEEN THE DOOR HEADER AND AUXILIARY WEATHERSTRIP.

#### CORRECTION:

1. CLEAN DOOR HEADER AT AUXILIARY WEATHERSTRIP LOCATION.

2. INSPECT DOOR HEADER FOR RUB MARKS OR INDICATION OF CONTACT WITH AUXILIARY WEATHERSTRIP.

3. APPLY 3M 5430 SQUEAK REDUCTION TAPE OR EQUIVALENT TO AUXILIARY WEATHERSTRIP AT POINT OF CONTACT.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T3463 LABOR TIME: 0.3 HRS.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.