AERO MOULDING WAVY UPPER EDGE LOOSE FIT SERVICE PROCEDURE. Pontiac Sunbird 1991

For 1990-2009 cars

# AERO MOULDING WAVY UPPER EDGE LOOSE FIT SERVICE PROCEDURE

#### SUBJECT: WAVY UPPER EDGE/LOOSE OR NO ENGAGEMENT OF CLIP ON AERO MOULDING (REMOVE MATERIAL FORM MOULDING)

#### VEHICLES AFFECTED: 1991 CHEV Z24 'J'

#### CONDITION:

------------- Some 1991 Chevrolet Z-24 models may have Aero Mouldings that exhibit one of the following conditions:

1. Wavy upper edge 2. Loose or no engagement of clip

#### CORRECTION:

------------ Condition #1 refer to illustration and situation #1. Remove 2.0 mm (3/32") from the top edge of the clip.

Condition #2 refer to illustration and situation #2. Remove 2.0 mm (3/32") from the stud openings as indicated and reinstall using 2 self drilling screws at the locations indicated.

Use the most applicable Labour Operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.