LABOR TIME GUIDE REVISIONS DEC - FEB 88 MODELS, ALL. Pontiac Sunbird 1988

For 1990-2009 cars

# LABOR TIME GUIDE REVISIONS DEC - FEB 88 MODELS, ALL

This bulletin addresses changes to the published Pontiac Labor Time Guide, December through February changes attached. These changes are the result of dealer "Requests for Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future revisions as printed, and at that time it is recommended that you dispose of the paper copy.

In the case of past model year updates, it is recommended that this bulletin be retained with the appropriate model year labor time guide as a complete revision will not be provided.

A-3 REQUEST FOR REVIEW ------------------ VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N P T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW EFGM NRSX JKP ------------------------------------------------------------------------------ PANEL, REAR END NOTE: Applicable model years: 1985-1988 INC: Removal of panel and lamp assys. on N series COLOR COAT A2780 .9 GE REFINISH A2790 1.1 GE ADD: A- W/Clear coat paint... .2 CA ------------------------------------------------------------------------------ HOUSING ASSEMBLY, SUNROOF (MODULE)-REPLACE B2780 NOTE: Applicable model years: 1984-1988 SEAL,SUNROOF SLIDING GLASS-REPLACE B2770 1.2 ------------------------------------------------------------------------------ SPOILER - R&R OR REPLACE NOTE: Applicable model years: 1987-1988 ONE PIECE B5608 .4 ------------------------------------------------------------------------------ COVER, HIGH LEVEL STOP LAMP - REPLACE B5650 .4 NOTE: Applicable model years: 1987-1988 ADD: A- To Color Coat...... .2 CA ------------------------------------------------------------------------------ MOLDING, FENDER - R&R OR REPLACE RIGHT SIDE B7466 .2 LEFT SIDE B7466 .2 NOTE: Applicable model years: 1987-1988 ------------------------------------------------------------------------------ MOLDING, ROOF RAIL DRIP SCALP-R&R OR REPLACE RIGHT B7620 .4 LEFT B7621 .4 ADD: A-To Replace Retainer Exc 2 Door and Wagons.. 1.5 2 Door ................ 1.8 Wagon ................. 2.7 ------------------------------------------------------------------------------

A-4 REQUEST FOR REVIEW ------------------

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N P T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW EFGM NRSX JKP ------------------------------------------------------------------------------ REGULATOR, FRONT DOOR WINDOW-R&R OR REPLACE NOTE: Applicable model years: 1987-1988 RIGHT MANUAL C0180 LEFT MANUUL C0181 2 DOOR .9 4 DOOR .9 RIGHT POWER C0182 LEFT POWER C0183 2 DOOR 1.0 4 DOOR 1.0 ------------------------------------------------------------------------------ CABLE, AIR DISTRIBUTION- R&R OR REPLACE NOTE: Applicable model years: 1987-1988 AIR CONDITIONING TEMPERATURE D0447 1.1 ------------------------------------------------------------------------------ CONDENSER - REPLACE D3140 1.3 NOTE: Applicable model years: 1987-1988 ------------------------------------------------------------------------------ GEAR, CAMSHAFT TIMING - REPLACE J0840 7.6 NOTE: Applicable model years: 1985-87 w/L-4 ------------------------------------------------------------------------------ MANIFOLD, EXHAUST - REPLACE LEFT BANK J0101 1.2 NOTE: Applicable model years: 1985-87 w/V-6 ------------------------------------------------------------------------------ PUSH ROD - REPLACE BOTH BANKS J0587 1.3 NOTE: Applicable model years: 1987-88 ------------------------------------------------------------------------------ CAMSHAFT - REPLACE J0850 7.0 NOTE: Applicable model years: 1985-87 w/V-6 ADD: A-With A/C ............. .3 B-To Replace Camshaft 1.4 Bearings ............. ------------------------------------------------------------------------------ MODULE, LOW COOLANT J3037 .4 .4 - REPLACE NOTE: Applicable model years: 1987-88 ------------------------------------------------------------------------------

A-5 REQUEST FOR REVIEW ------------------

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N P T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW EFGM NRSX JKP ------------------------------------------------------------------------------ RESERVOIR, RADIATOR COOLANT - REPLACE J3260 .5 NOTE: Applicable model years: 1987-88 (Correction to the misprint in the SEPTEMBER/OCTOBER Bulletin) ADD: A- With A/C............... .1 ------------------------------------------------------------------------------ SWITCH - REPLACE DOOR WINDOW FRONT N2142 .5 NOTE: Applicable model years: 1985-1986 REAR COMPARTMENT LID AJAR N2386 .3 NOTE: Applicable model years: 1984-1988 WINDSHIELD WASHER FLUID LEVEL N2590 .2 .2 NOTE: Applicable model years: 1985-1988 ------------------------------------------------------------------------------ RELAY, TERMINAL BOARD AND/OR TIMING SWITCH, WINSHIELD WIPER MOTOR - REPLACE N3580 .3 NOTE: Applicable model years: 1987-1988 ------------------------------------------------------------------------------ MEMORY SEAT SYSTEM COMPONENTS - REPLACE NOTE: Applicable model years: 1987-1988 MODULE N5510 .5 SWITCH N5520 .2 ------------------------------------------------------------------------------ PANEL, FRONT DOOR OUTER - REPLACE NOTE: Applicable model years: 1985-1988 RIGHT S0800 LEFT S0801 2 DOOR 1.9 ------------------------------------------------------------------------------

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.