CLUTCH PEDAL FREE-PLAY ADJUSTMENT. Pontiac Sunbird 1985

For 1990-2009 cars

# CLUTCH PEDAL FREE-PLAY ADJUSTMENT

1984 "J" AND EARLY 1985 "N" MODELS ARE EQUIPPED WITH A CABLE CONTROLLED CLUTCH MECHANISM. CLUTCH PEDAL FREE-PLAY ADJUSTMENT IS REQUIRED EVERY 5,000 MILES OR LESS. THE CLUTCH ADJUSTMENT IS PERFORMED BY SIMPLY LIFTING UP ON THE CLUTCH PEDAL. 1985 "J" MODELS ARE EQUIPPED WITH A HYDRAULIC CLUTCH AND DO NOT REQUIRE A FREE-PLAY ADJUSTMENT. THE HYDRAULIC CLUTCH IS ALSO SCHEDULED FOR MID-YEAR PRODUCTION OF THE 1985 "N".

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.