SERVICE MANUAL UPDATE STARTER REMOVE AND REPLACE. Pontiac Sunbird 1987

For 1990-2009 cars

# SERVICE MANUAL UPDATE STARTER REMOVE AND REPLACE

#### VEHICLES AFFECTED: LH8, LA5 (1.8L) AND LT2, LT3 (2.0L) ENGINES ON "J" CARLINES, BOTH MANUAL AND AUTOMATIC TRANSAXLES

This bulletin provides a new procedure to remove and replace starters on 1.8L and 2.0L engines on "J" carlines.

STARTER J CAR (Manual and Automatic Trans.)

A. 1. Negative battery cable. 2. Blower motor wires. 3. Blower motor. 4. Starter wiring. 5. Rear starter brace. 6. Loom strap at upper starter bolt. 7. Upper starter bolt. 8. Raise vehicle. 9. Transaxle strut (automatic). 10. Lower starter bolt. 11. Lower vehicle. 12. Starter (through blower motor opening).

B. 1. Starter (through blower motor opening). 2. Upper starter bolt. I. Requires two men: One on passenger side to hold starter in place; another on driver's side to start bolt. 3. Raise vehicle. 4. Lower starter bolt. 5. Transaxle strut (automatic). 6. Lower vehicle. 7. Loom strap at upper starter bolt. 8. Rear starter brace. 9. Starter wiring. 10. Blower motor. 11. Blower motor wires. 12. Negative battery cable.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.