For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the convenience net from the retainers.
3. Remove the bolt/screw from the upper convenience net retainer.
4. Remove the upper convenience net retainer from the body.

### Installation Procedure

1. Install the upper convenience net retainer to the body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt/screw to the upper convenience net retainer.

Tighten
Tighten the bolt/screw to 2.0 N·m (18 lb in).

3. Install the convenience net to the retainers.
4. Close the liftgate.