For 1990-2009 cars

#### No Reverse

Checks | Cause
--- | ---
Oil Pressure | Refer to Causes of High or Low Pressure
Reverse Servo |

• | Misassembled servo

• | Damaged piston or seal

• | Missing cushion spring or retainers

Oil Pump Assembly | Refer to No Drive in Drive Range
Drive Link Assembly | Refer to No Drive in Drive Range
Reverse Band |

• | Burned or damaged reverse band

• | Mislocated band apply pin

Input Clutch | Refer to No Drive in Drive Range
1-2 Shift Solenoid valve or TCC Solenoid valve | Malfunctioned or walked out solenoid
Reverse Reaction Drum | Damaged splines
Input Sprag | Refer to No Drive in Drive Range
Input and Reaction Carriers | Refer to No Drive in Drive Range