For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Remove the front door sill plate. Refer to Front Side Door Sill Plate Replacement .
2. Remove the cowl side trim panel retainers using the J 38778 .
3. Remove the cowl side trim panel from the vehicle.

### Installation Procedure

1. Install the cowl side trim panel to the vehicle by aligning the trim panel with the slots in the cowl.
2. Install the cowl side trim panel retainers by pushing in on the panel to secure.
3. Install the front door sill plate. Refer to Front Side Door Sill Plate Replacement .