For 1990-2009 cars

## Steering Wheel Replacement Pontiac

### Removal Procedure

#### Tools Required

• | J 1859-A Steering Wheel Puller

• | J 42578 Steering Wheel Puller Legs

1. Turn the ignition OFF.
2. Remove the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
3. If there are no alignment mark on the steering wheel hub, scribe an alignment mark on the steering wheel hub in line with the mark on the steering shaft.
4. Loosen the steering wheel nut.
5. Position the steering wheel nut flush with the end of the steering column shaft.
6. Use the J 1859-A and the J 42578 in order to loosen the steering wheel.
7. Remove the J 1859-A and the J 42578 from the steering wheel.
8. Disconnect the steering wheel controls electrical connector (if equipped).
9. Disconnect the horn switch lead from the steering hub.
10. Remove the steering wheel nut.
11. Remove the steering wheel from the steering shaft.
12. Remove the steering wheel controls and the steering wheel controls harness from the steering wheel (if equipped). Refer to Steering Wheel Control Switch Assembly Replacement .

### Installation Procedure

1. Install the steering wheel controls and the steering wheel controls harness to the steering wheel (if equipped). Refer to Steering Wheel Control Switch Assembly Replacement .
2. Route the SIR connector through the steering wheel.
3. Align the mark on the steering wheel with the mark on the steering shaft.
4. Install the steering wheel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops 3 N·m (27 lb in) of torque (drag) against its counterpart prior to the fastener seating.

If the fastener does not meet these criteria, REPLACE the fastener.
5. Install the steering wheel nut.

Tighten
Tighten the steering wheel nut to 45 N·m (33 lb ft).

6. Connect the horn switch lead to the steering hub.
7. Connect the steering wheel controls electrical connector (if equipped).
8. Install the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
9. Verify that the steering wheel controls operate properly (if equipped).
10. Verify that the horn operates properly.

## Steering Wheel Replacement Chevrolet/Oldsmobile

### Removal Procedure

#### Tools Required

J 1859-A Steering Wheel Puller

1. Turn the ignition OFF.
2. Remove the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
3. If there are no alignment marks on the steering wheel, scribe an alignment mark on the steering wheel hub in line with the mark on the steering shaft.
4. Loosen the steering wheel nut.
5. Position the steering wheel nut flush with the end of the shaft.
6. Use the J 1859-A in order to loosen the steering wheel.
7. Remove the J 1859-A from the steering wheel.
8. Disconnect the steering wheel controls electrical connector (if equipped).
9. Disconnect the horn switch lead from the steering hub.
10. Remove the steering wheel nut.
11. Remove the steering wheel from the steering shaft.
12. Remove the steering wheel controls and the steering wheel controls harness from the steering wheel (if equipped). Refer to Steering Wheel Control Switch Assembly Replacement .

### Installation Procedure

1. Install the steering wheel controls and the steering wheel controls harness to the steering wheel (if equipped). Refer to Steering Wheel Control Switch Assembly Replacement .
2. Route the SIR connector through the steering wheel.
3. Align the mark on the steering wheel with the mark on the steering shaft.
4. Install the steering wheel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops 3 N·m (27 lb in) of torque (drag) against its counterpart prior to the fastener seating.

If the fastener does not meet these criteria, REPLACE the fastener.
5. Install the steering wheel nut.

Tighten
Tighten the steering wheel nut to 45 N·m (33 lb ft).

6. Connect the horn switch lead to the steering hub.
7. Connect the steering wheel controls electrical connector (if equipped).
8. Install the inflator module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
9. Verify that the steering wheel controls operate properly (if equipped).
10. Verify that the horn operates properly.