For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Perform the self-diagnostic tests on the driver information display. Go to Driver Information System Check . | The display segments light for 2 seconds, then turn off for 2 seconds. | DIC Display Inoperative
2 |

1. Turn the ignition switch to the ON position.
2. Toggle the display MODE button to temperature/compass.

• | The outside temperature is displayed.

• | The display shows a compass readout on one side of the display, when the trip functions are not displayed.

• | Driver Information Center (DIC) Temperature Display Always Reads SC

• | Driver Information Center (DIC) Temperature Display Always Reads OC

• | Driver Information Center (DIC) Temperature Display Always Reads One Value

• | Driver Information Center (DIC) Temperature Display Inaccurate

• | Driver Information Center (DIC) Compass Inaccurate or CAL Displayed

3 | Toggle the display MODE button to the trip computer functions. | The driver information display shows one of the following functions:

• | Average Fuel Economy

• | Instantaneous Fuel Economy

• | Trip Range

• | Fuel Used

• | Average Speed

• | Driver Information Center (DIC) Always Displays Dashes

• | Driver Information Center (DIC) Always Displays E

4 |

1. Turn on the park lamps.
2. Adjust the dimmer switch for the headlamp and instrument panel lamp assembly.

• | The display dims.

• | The driver information display brightness varies while adjusting the headlamp and instrument lamp dimmer switch.

The display dims

Driver Information Center (DIC) Display Does Not Dim

5 |

1. Set the display to one of the following modes:

• | AVE ECON

• | FUEL USED

• | AVG SPEED

2. Press the MODE button and the ENGLISH/METRIC button simultaneously for 2 seconds.

1. The display shows all of the segments ON for a period of 2 seconds.
2. The display resets the following modes if you are in that function:

• | AVE ECON

• | FUEL USED

• | AVG SPEED

Driver Information Center (DIC) Switch Inoperative - Reset

6 | Press the ENGLISH/METRIC switch. | The display units change from English to metric. | Driver Information Center (DIC) Switch Inoperative - English/Metric
7 | Turn OFF the ignition switch, then turn ON the ignition switch. | The display retains the last request mode before turning off the ignition. | Driver Information Center (DIC) Display Does Not Retain Last Request Mode
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.