For 1990-2009 cars

Condition | Probable Cause | Correction
--- | --- | ---
The sliding door is hard to open or close. |

1. Inspect the tracks for foreign objects, weld flash or metal burrs.
2. Binding or misaligned sliding door.

1. Clear foreign objects, clean or replace the track.
2. Inspect track for pinched areas, weld flash and burrs.

Refer to Roller Track Replacement - Sliding Door Upper for upper track replacement, Roller Track Replacement - Sliding Door Center for center track replacement in Doors.

3. Align the sliding door.

Refer to Rear Side Door Up/Down Adjustment for up/down adjustment, Rear Side Door Front Edge In/Out Adjustment for front edge in/out adjustment, or Rear Side Door Rear Edge In/Out Adjustment for rear edge in/out adjustment in Doors.

Windnoise or water leaks. |

1. Improper weather-strip position.
2. Improper sliding door alignment.

1. Reposition the weather-strip.
2. Align the sliding door.

Refer to Rear Side Door Up/Down Adjustment for up/down adjustment, Rear Side Door Front Edge In/Out Adjustment for front edge in/out adjustment, or Rear Side Door Rear Edge In/Out Adjustment for rear edge in/out adjustment in Doors.

Improper fit of the sliding door. | Improper fit, flushness or gaps. | Align the sliding door. Refer to Rear Side Door Up/Down Adjustment for up/down adjustment, Rear Side Door Front Edge In/Out Adjustment for front edge in/out adjustment, or Rear Side Door Rear Edge In/Out Adjustment for rear edge in/out adjustment in Doors.
Sliding door jerks, clunks or bounces on operation. |

1. Inspect the tracks for foreign objects.
2. Roller damage.
3. Roller to track bind.
4. Improperly adjusted cable tension.

1. Clear foreign object, clean or replace the track. Refer to Roller Track Replacement - Sliding Door Upper for upper track replacement, Roller Track Replacement - Sliding Door Center for center track replacement in Doors.
2. Replace the rollers.
3. Align the door. Refer to Rear Side Door Up/Down Adjustment for up/down adjustment, Rear Side Door Front Edge In/Out Adjustment for front edge in/out adjustment, or Rear Side Door Rear Edge In/Out Adjustment for rear edge in/out adjustment in Doors.
4. Adjust the cable tension. Refer to Rear Side Door Actuator Cable Tension Adjustment .