For 1990-2009 cars

#### Tools Required

J 41131 Engine Tilt Strap

1. Remove the throttle body air inlet duct. Refer to Air Cleaner Element Replacement in Engine Controls - 3.4L.
2. Set the park brake.
3. Shift the transaxle into Neutral.
4. Remove the engine mount strut bolts. Swing the engine mount struts aside. Refer to Engine Mount Strut Replacement .
5. Install the J 41131 .
6. Rotate the engine forward for component access.
7. Tighten the J 41131 .