For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to ACCY or RUN.
2. Set the wiper/washer switch to DELAY.

The wiper makes one complete sweep, then pauses or approximately 5 seconds before making the next sweep. The delay time is preset and not adjustable.

Rear Wiper Inoperative .

2 | Set the wiper switch to WASH. | The washer sprays the window as long as the switch is held on WASH. The wipers run continuously while the washer is on. | Rear Washer Inoperative .
3 | Set the wiper switch to OFF. | The wiper completes the last sweep, then parks. | Rear Wiper Always On .