For 1990-2009 cars

1. Remove the steering column tilt head assembly. Refer to Steering Column Tilt Head Housing - Disassemble - Off Vehicle .
2. Remove the key alarm connector (1) from the lock module assembly (2).
3. Remove the 2 tapping screws from the ignition key alarm switch assembly (3).
4. Let both parts hang freely.
5. Remove the park lock cable assembly (1) from the lock module assembly.
6. Remove 3 pan head tapping screws (2) from the lock module assembly (1).
7. Remove the lock module assembly (1).