For 1990-2009 cars

# SER.MAN.UPDATE SEC.10 SEATBELT CHILD SEAT TOP STRAP ANCHOR

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 10 SAFETY BELTS CHILD SEAT TOP STRAP ANCHOR (ADDENDUM)

#### VEHICLES AFFECTED: 1990-91 U-VANS W/OUT 3RD ROW SEATING

#### SECTION 10-11

Child seat top strap anchor plate installation 2nd. row seating, bench or bucket seat LH or RH outboard position only.

1. From rear of vehicle with liftgate open, mark reference point that is 380mm (15 inches) forward of front edge of rear floor trim plate and 165mm (6.5 inches) inward from lower wheelhouse jack storage door (RH side) or ELC door (LH side).

2. At reference marks cut an X through carpet to expose weld nut on floor.

3. Install anchor bolt through anchor plate to weld nut, tighten bolt to 42 N.m. (31 ft.lbs.) .

4. Install child seat top strap retaining hook to anchor plate.

#### Note: Installation of the anchor plate is not required on vehicles equipped with 3rd row seating. With the child seat in the correct position in the 2nd. row, the top strap retaining hook and strap should be attached to the 3rd. row seat forward floor anchor plate pin.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.