For 1990-2009 cars

### Removal Procedure

1. Remove the IP ashtray. Refer to Ashtray Replacement .
2. Use a small, flat-bladed tool in order to depress the retainers on the IP power accessory port.
3. Remove the IP power accessory port from the ashtray.

### Installation Procedure

1. Press in on the IP power accessory port until the port is fully seated in order to install the IP power accessory port to the ashtray.
2. Install the IP ashtray. Refer to Ashtray Replacement .