For 1990-2009 cars

Table 1: | Interior Lamp and Multi-function Switch C1
Table 2: | Interior Lamp and Multi-function Switch C3
Table 3: | Interior Lamp and Multi-function Switch C4
Table 4: | In-line Connector C397
Table 5: | In-line Connector C398
Table 6: | In-line Connector C308
Table 7: | In-line Connector C200

#### Interior Lamp and Multi-function Switch C1

Connector Part Information |

• | 12162502

• | 8-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 650 | Ground
2 | GRY | 8 | Interior lamp dim signal
3-4 | -- | -- | Not used
5 | DK BLU | 1393 | Courtesy lamps feed-protected battery
6-7 | -- | -- | Not used
8 | PPL | 328 | Interior lamp override switch output

#### Interior Lamp and Multi-function Switch C3

Connector Part Information |

• | 12041301

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 650 | Ground
C | LT BLU | 1894 | Power sliding door switch signal
D | BLK/WHT | 1896 | Power sliding door system switch signal
E-H | -- | -- | Not Used

#### Interior Lamp and Multi-function Switch C4

Connector Part Information |

• | 12047976

• | 8-Way F Metri-Pack 280 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 650 | Ground
C | BLK | 902 | Rear quarter window switch-open
D | BRN | 901 | Rear quarter window switch-close
E | BRN | 741 | Fused ignition 3 feed
F | ORN | 110 | Sunroof switch signal-close
G | DK BLU | 128 | Sunroof switch return
H | BRN | 100 | Sunroof switch signal-open

#### In-line Connector C397

Connector Part Information |

• | 12129489

• | 3-Way F Metri-Pack 280 Flexlock Series (BLK)

Connector Part Information

• | 12129490

• | 3-Way M Metri-Pack 280 Flexlock Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | ORN | 110 | Sunroof switch signal-close | A | ORN | 110 | Sunroof switch signal-close
B | BRN | 100 | Sunroof switch signal-open | B | BRN | 100 | Sunroof switch signal-open
C | DK BLU | 128 | Sunroof switch return | C | DK BLU | 128 | Sunroof switch return

#### In-line Connector C398

Connector Part Information |

• | 12020397

• | 3-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | 541 | Fused ignition 3 feed | A | BRN | 541 | Fused ignition 3 feed
B | -- | -- | Not used | B | -- | -- | Not used
C | BLK | 650 | Ground | C | BLK | 650 | Ground

#### In-line Connector C308

Connector Part Information |

• | 12092249

• | 23-Way F ACT 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23-Way M ACT 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 901 | Rear quarter window switch-close | A | BLK | 901 | Rear quarter window switch-close
B | LT GRN/BLK | 735 | Ambient air temperature sensor signal | B | LT GRN/BLK | 735 | Ambient air temperature sensor signal
C | DK GRN | 389 | Vehicle speed signal | C | DK GRN | 389 | Vehicle speed signal
D | -- | -- | Not used | D | YEL | 136 | Fuel level input
E | BLK/WHT | 1896 | Power sliding door system switch signal | E | BLK/WHT | 1896 | Power sliding door system switch signal
F | TAN | 800 | UART serial data communication | F | TAN | 800 | UART serial data communication
G | GRY | 8 | Interior lamp dim signal | G | GRY | 8 | Interior lamp dim signal
H | YEL | 43 | Fused accessory feed | H | YEL | 43 | Fused accessory feed
J | BLK | 1550 | Ground | J | BLK | 1550 | Ground
K | BRN | 741 | Fused ignition 3 feed | K | BRN | 741 | Fused ignition 3 feed
L | -- | -- | Not used | L | -- | -- | Not used
M | GRY/BLK | 308 | Park lamp switch output-parklamps ON | M | GRY/BLK | 308 | Park lamp switch output-parklamps ON
N | ORN | 640 | Fused battery feed | N | ORN | 640 | Fused battery feed
P | -- | -- | Not used | P | -- | -- | Not used
R | LT GRN | 24 | Backup lamp feed | R | -- | -- | Not used
S | GRY/BLK | 690 | Courtesy lamp control | S | GRY/BLK | 690 | Courtesy lamp control
T | -- | -- | Not used | T | -- | -- | Not used
U | LT BLU | 1894 | Power sliding door switch signal | U | LT BLU | 1894 | Power sliding door switch signal
V | -- | -- | Not used | V | -- | -- | Not used
W | DK BLU | 1393 | Courtesy lamps feed-protected battery | W | DK BLU | 1393 | Courtesy lamps feed-protected battery
X | PPL | 328 | Interior lamp override switch output | X | PPL | 328 | Interior lamp override switch output
Y | BRN | 541 | Fused ignition 3 feed | Y | BRN | 541 | Fused ignition 3 feed
Z | BRN | 902 | Rear quarter window switch-open | Z | BLK | 902 | Rear quarter window switch-open

#### In-line Connector C200

Connector Part Information |

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | ORN | 340 | Fused battery feed | A1 | ORN | 340 | Fused battery feed
A2 | LT BLU | 1894 | Power sliding door switch signal | A2 | LT BLU | 1894 | Power sliding door switch signal
A3-A6 | -- | -- | Not used | A3-A6 | -- | -- | Not used
A7 | GRY | 120 | Fuel pump motor feed | A7 | GRY | 120 | Fuel pump motor feed
A8 | BRN | 141 | Fused ignition 3 feed | A8 | BRN | 141 | Fused ignition 3 feed
A9 | BRN | 541 | Fused ignition 3 feed | A9 | BRN | 541 | Fused ignition 3 feed
B1 | -- | -- | Not used | B1 | -- | -- | Not used
B2 | LT GRN | 275 | Transaxle range switch feed-PARK | B2 | LT GRN | 275 | Transaxle range switch feed-PARK
B3 | GRY/BLK | 690 | Courtesy lamp control | B3 | GRY/BLK | 690 | Courtesy lamp control
B4 | ORN | 1240 | Fused battery feed | B4 | ORN | 1240 | Fused battery feed
B6-B7 | -- | -- | Not used | B6-B7 | -- | -- | Not used
B8 | DK BLU | 1393 | Courtesy lamps feed-protected battery | B8 | DK BLU | 1393 | Courtesy lamps feed-protected battery
B9 | -- | -- | Not used | B9 | -- | -- | Not used
C1 | PPL | 328 | Interior lamp override switch output | C1 | PPL | 328 | Interior lamp override switch output
C2 | PNK | 1139 | Fused ignition 1 feed | C2 | PNK | 1139 | Fused ignition 1 feed
C3 | BRN | 358 | Airbag indicator lamp output | C3 | BRN | 358 | Airbag indicator lamp output
C4 | -- | -- | Not used | C4 | -- | -- | Not used
C6 | LT GRN/BLK | 735 | Ambient air temperature sensor signal | C6 | LT GRN/BLK | 735 | Ambient air temperature sensor signal
C7 | DK GRN | 389 | Vehicle speed signal (VSS) | C7 | DK GRN | 389 | Vehicle speed signal (VSS)
C8 | -- | -- | Not used | C8 | -- | -- | Not used
C9 | PNK | 1039 | Fused ignition 1 feed | C9 | PNK | 1039 | Fused ignition 1 feed