For 1990-2009 cars

### Removal Procedure

1. Remove the indicator.
2. Remove the nut from the upper fluid filler tube bracket on the stud of the EGR.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
4. Remove the three-way catalytic converter pipe. Refer to Catalytic Converter Replacement in Engine Exhaust.
5. Remove the power steering gear heat shield. Refer to Power Steering Gear Heat Shield Replacement in Power Steering Gear and Pump.
6. Remove the fluid filler tube bracket bolt from the fluid filler tube bracket.
7. Remove the fluid filler tube.

### Installation Procedure

Important: Do NOT place the fluid filler tube seal on the fluid filler tube when installing the tube or damage to the seal will result.

1. Install the fluid filler tube seal in the transaxle.
2. Position the fluid filler tube.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fluid filler tube bracket bolt through the fluid filler tube bracket.

Tighten
Tighten the fluid filler tube bracket bolt to 13 N·m (115 lb in).

4. Install the power steering gear heat shield. Refer toPower Steering Gear Heat Shield Replacement in Power Steering Gear and Pump.
5. Install the three-way catalytic converter pipe. Refer to Catalytic Converter Replacement in Engine Exhaust.
6. Lower the vehicle.
7. Install the fluid filler tube bracket nut through the upper fluid filler tube bracket to the stud on the EGR.

Tighten
Tighten the fluid filler tube bracket nut to 13 N·m (115 lb in).

8. Install the indicator.
9. Adjust the fluid level. Refer to the following information.

• | Transmission Fluid Check

• | Fluid and Lubricant Recommendations in Maintenance and Lubrication

• | Approximate Fluid Capacities in Maintenance and Lubrication

10. Inspect for proper completion of the repairs.
11. Inspect for proper fluid level.
12. Inspect for fluid leaks.