For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Open the front door.
2. Use the J 38778 in order to remove the push-in retainers from the front door bottom auxiliary weatherstrip.
3. Remove the front door bottom auxiliary weatherstrip from the front door.

### Installation Procedure

1. Install the front door bottom auxiliary weatherstrip to the front door.
2. Stretch the front door bottom auxiliary weatherstrip in order to align the push-in retainers to the holes in the front door.
3. Install the push-in retainers to the front door bottom auxiliary weatherstrip.
4. Close the front door.